**Assignment Submission**

**Heading: Networking Lab 10**

**Approach:**

* Configured VLAN1 IP addresses and MAC addresses on switches.
* Enabled interfaces and adjusted port states.
* Configured PC IP addresses according to VLAN1.

**Solution:**

Senior Switch:

- VLAN1 IP address and MAC address were configured, and the interface was enabled.

- FastEthernet 0/1 was brought up.

- PC IP addresses were configured according to VLAN1.

Junior Switch:

- VLAN1 IP address and MAC address were configured, and the interface was enabled.

- PC IP addresses were configured according to VLAN1.

Admin Switch:

- VLAN1 IP address and MAC address were configured, and the interface was enabled.

- VLAN20 was shutdown.

- PC IP addresses were configured according to VLAN1.