**Assignment Submission**

**Heading: Networking Lab 9**

**Approach:**

* Configured enable secret password on the Senior switch.
* Assigned IP addresses and enabled VLAN1 interface on both Admin and Senior switches.

**Solution:**

Senior Switch:

- Enable secret password "hack" was configured.

- VLAN1 interface was configured with IP address and enabled.

Admin Switch:

- VLAN1 interface was configured with IP address and enabled.